**APPENDIX AA
COMMENTS TEMPLATE**

**CPR 183/F11**

|  |  |
| --- | --- |
| **Title:** | DKS 2991, Almond kernels—Specification |
| **Document Type:** | Draft Kenya standard |
| **Dates:** | Opening date | 2024/02/01 |
| Closing date | 2024/04/01 |
| **Recipient** | Mercy Ndirangu (ndirangum@kebs.org) |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Organization | Clause | Paragraph/ Figure/Table | Type of comment (General/Technical /Editorial) | COMMENTS | Proposed Change | TC Observation(s) |
| KEBS | 12(5) | Page 62 | Tech | (5) If an owner uses electric fencing, it shall be installed in accordance with KS - 04 - 646 Part 2 of 1987 (Specification for Electric Fence Controllers - Part 1: Mains Operated. (Withdrawn)). You can’t reference a withdrawn standard unless it still applies under the circumstances. | Reference the correct standard KS IEC 60335-2-76:2018, Household and similar electrical appliances - Safety - Part 2-76: Particular requirements for electric fence energizers |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |   |