APPENDIX DD  
ADOPTION PROPOSAL FORM

**CPR183/F12**

**KENYA BUREAU OF STANDARDS**

|  |  |  |
| --- | --- | --- |
| **Document Type:** | **Adoption proposal** | |
| **Dates:** | Circulation date | Closing date |
| 30th January 2024 | 29th February 2024 |
| **TC Secretary** | **This form shall be filled, signed and returned to Kenya Bureau of Standards for the attention of Eng. Leonard Kipchumba (**[kipchumbal**@kebs.org**](mailto:kipchumbal@kebs.org)**)** | |

The Kenya Bureau of Standards intends to adopt the International Standards as detailed here below:

**KEBS 112: CONTAINERS AND TANKS**

1. **Number:** ISO 3807:2013 to replace KS ISO 3807-1:2000

**Title:** Gas cylinders - Acetylene cylinders

Basic requirements and type testing

**Scope:**

This International Standard specifies the basic and type testing requirements for acetylene cylinders with and without fusible plugs with a maximum nominal water capacity of 150 l and requirements regarding production/batch test procedures for manufacturing of acetylene cylinders with porous material.

It does not include details of the design of the cylinder shell; these are specified, for example, in ISO 9809-1, ISO 9809-3, ISO 4706 and ISO 7866.

NOTE The limitation to 150 l is derived from the definition for cylinder in the UN Model Regulations. However, in practice acetylene cylinders in general have lower water capacities than 150 l.

<https://www.iso.org/obp/ui/en/#iso:std:iso:3807:ed-2:v2:en>

1. **Number:** ISO 7225:2005/Amd 1:2012

**Title:** Gas cylinders

Precautionary labels

Amendment 1

**Scope:**

This International Standard specifies the design, content (i.e. hazard symbols and text) and application of precautionary labels intended for use on individual gas cylinders containing single gases or gas mixtures. Labels for cylinders of bundles and labels for bundles are not covered by this International Standard.

<https://www.iso.org/obp/ui/en/#iso:std:iso:7225:ed-2:v1:amd:1:v1:en>

We are therefore seeking views from potential users in respect of the same. The Standard is available at the Kenya Bureau of Standards Information Centre. Please tick and fill your preference of the listed option. (If the spaces provided are not enough, please attach a separate sheet of paper).

Adoption acceptable as presented

...............................................................................................................................

...............................................................................................................................

Adoption proposal not acceptable because of the reason(s) below

...............................................................................................................................

...............................................................................................................................

Our Recommendations are as follows

...............................................................................................................................

...............................................................................................................................

Name and Signature (of respondent): ................................................

Position (of respondent): .....................................

On behalf of ......................................................................................... (Name of organization)

Date .........................................................................

**NOTE:** Absence of any reply or comments shall be deemed to be an acceptance of the proposal for adoption and **shall constitute an approval vote**.